B D E F G H I P S T U V

## S

setGpio(int, GpioSetting.GpioPin, GpioObject) - Method in class tw.com.prolific.pl2303ghidsdk.HidToGpio
  PL23B3, PL23C3, and PL23D3 have some software controllable "General Purpose Input Output" control signal pin, you can use this API to control the status of these pin when the direction is output mode
setGpioDir(int, GpioSetting.GpioPin, GpioSetting.GpioDir) - Method in class tw.com.prolific.pl2303ghidsdk.HidToGpio
  PL23B3, PL23C3, and PL23D3 have some software controllable "General Purpose Input Output" control signal pin, you can use this API to control the direction of these pin
setI2cDeviceAddress(int, byte) - Method in class tw.com.prolific.pl2303ghidsdk.HidToI2c
  Sets I2C device address.
setI2cFrequency(int, byte) - Method in class tw.com.prolific.pl2303ghidsdk.HidToI2c
  Sets I2C frequency.
setSpiFrequency(int, byte, SpiSetting.SPI_MODE) - Method in class tw.com.prolific.pl2303ghidsdk.HidToSpi
  Sets spi frequency.
setUartConfig(int, UartObject) - Method in class tw.com.prolific.pl2303ghidsdk.HidToUart
  Sets UART config, the configurations included BaudRate, Data bit, stop bit, parity bit and Flow Control.
setXonXoffSymbol(int, byte, byte) - Method in class tw.com.prolific.pl2303ghidsdk.HidToUart
  Sets Software Flow Control byte (Xon/Xoff Symbol)
spiRead(int, SpiSetting.Select, byte[], int, int) - Method in class tw.com.prolific.pl2303ghidsdk.HidToSpi
  Read Binary Data from PL23D3 HidtoSpi chip.
spiReset(int) - Method in class tw.com.prolific.pl2303ghidsdk.HidToSpi
  Reset PL23D3 HidToSpi Chip configurations.
SpiSetting - Class in tw.com.prolific.pl2303ghidsdk
  The SPI Setting definitions, including CsControl, and Chip Select.
SpiSetting() - Constructor for class tw.com.prolific.pl2303ghidsdk.SpiSetting
SpiSetting.CsControl - Enum in tw.com.prolific.pl2303ghidsdk
SpiSetting.Select - Enum in tw.com.prolific.pl2303ghidsdk
SpiSetting.SPI_MODE - Enum in tw.com.prolific.pl2303ghidsdk
spiWrite(int, SpiSetting.Select, byte[], int, int) - Method in class tw.com.prolific.pl2303ghidsdk.HidToSpi
  Write Binary Data to PL23D3 HidtoSpi chip.
spiWriteRead(int, SpiSetting.Select, byte[], int, byte[], int, int) - Method in class tw.com.prolific.pl2303ghidsdk.HidToSpi
  Write Read Data to PL23D3 HidtoSpi chip.
StopBit - Variable in class tw.com.prolific.pl2303ghidsdk.UartObject

B D E F G H I P S T U V